**SUPPLIER FAI CHECKLIST**

* Part used for first article inspection has been identified.
* AS9102 forms have been used, all documentation is legible.
* Drawing notes are accounted for on the FAIR (First Article Inspection Report)
* All dimensions are accounted for on the FAIR, results are recorded and within specification.
* A ballooned/bubbled drawing has been provided when there are more than 20 reportable dimensions.
* If a dimensioned drawing was not provided by PZ a vendor supplied drawing is included.
* Certifications (COC) for any referenced materials or special processes on the drawing or parts list have been provided.
* Certifications (COC) for any commercial parts identified on the drawing or parts list have been provided.
* If there are lower level parts manufactured to a PZ drawing a separate FAI has been provided for these.
* Non-conformances have been identified and approved in advance of shipment.
* Documentation package has been provided with the shipment of the FAI part or sent electronically (preferred method) to the buyer or supplier quality at the time of shipment.